*HEADING
FEMUR 3D SIMPLIFICADO  20-Apr-98   11:03:02
*NODE, SYSTEM=R
*ELEMENT,TYPE=C3D4    ,ELSET=GR1
*ELEMENT,TYPE=C3D6    ,ELSET=GR2
*ELEMENT,TYPE=C3D8   ,ELSET=GR3
*ELEMENT,TYPE=C3D8,ELSET=EAPOYO
**
*ELSET,ELSET=MECANOB
GR1,GR2,GR3
**
*ELSET,ELSET=TODOE
GR1,GR2,GR3,EAPOYO
**
**
**
*NSET,NSET=APOYOS
*NSET,NSET=CARABDUC
*NSET,NSET=vastusla
*NSET,NSET=vastusme
*NSET,NSET=contactoandar
*NSET,NSET=contactodepie
*NSET,NSET=NBOUNDARY
APOYOS,CARABDUC,vastusla,vastusme,contactoandar,contactodepie
*ELSET,ELSET=FRON4
*NSET,NSET=TODON
**
*ELSET,ELSET=MITAD2
*ELSET,ELSET=MITAD2MECAN
**
**
**	MATERIALES
**
*SOLID SECTION,ELSET=TODOE,MATERIAL=MAT1
*MATERIAL, NAME=MAT1
*USER DEFINED FIELD
*USER MATERIAL, CONSTANTS=16
*DEPVAR
**
*INITIAL CONDITIONS,TYPE=FIELD
**
*BOUNDARY
APOYOS,1,3
**
**
*AMPLITUDE,DEFINITION=TABULAR,INPUT=47,NAME=LC1
*AMPLITUDE,DEFINITION=TABULAR,INPUT=46,NAME=LC3
*STEP,AMPLITUDE=STEP,INC=52
*STATIC,DIRECT
1,52
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contactoandar,1,-35.3866666667
contactoandar,2,-51.895
contactoandar,3,-166
**APOYADO
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contactodepie,1,-7.68166666667
contactodepie,2,-50.1216666667
contactodepie,3,-184
*RESTART,WRITE,FREQUENCY=52
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=4
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
*STEP,AMPLITUDE=STEP,INC=52
*STATIC,DIRECT
1,52
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contactoandar,1,-35.3866666667
contactoandar,2,-51.895
contactoandar,3,-166
**APOYADO
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contactodepie,1,-7.68166666667
contactodepie,2,-50.1216666667
contactodepie,3,-184
*RESTART,WRITE,FREQUENCY=52
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=4
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
*STEP,AMPLITUDE=STEP,INC=52
*STATIC,DIRECT
1,52
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contactoandar,1,-35.3866666667
contactoandar,2,-51.895
contactoandar,3,-166
**APOYADO
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contactodepie,1,-7.68166666667
contactodepie,2,-50.1216666667
contactodepie,3,-184
*RESTART,WRITE,FREQUENCY=52
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=4
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
*STEP,AMPLITUDE=STEP,INC=52
*STATIC,DIRECT
1,52
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contactoandar,1,-35.3866666667
contactoandar,2,-51.895
contactoandar,3,-166
**APOYADO
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contactodepie,1,-7.68166666667
contactodepie,2,-50.1216666667
contactodepie,3,-184
*RESTART,WRITE,FREQUENCY=52
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=4
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
*STEP,AMPLITUDE=STEP,INC=52
*STATIC,DIRECT
1,52
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contactoandar,1,-35.3866666667
contactoandar,2,-51.895
contactoandar,3,-166
**APOYADO
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contactodepie,1,-7.68166666667
contactodepie,2,-50.1216666667
contactodepie,3,-184
*RESTART,WRITE,FREQUENCY=52
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=4
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
*STEP,AMPLITUDE=STEP,INC=52
*STATIC,DIRECT
1,52
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contactoandar,1,-35.3866666667
contactoandar,2,-51.895
contactoandar,3,-166
**APOYADO
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contactodepie,1,-7.68166666667
contactodepie,2,-50.1216666667
contactodepie,3,-184
*RESTART,WRITE,FREQUENCY=52
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=4
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**