*HEADING
FEMUR 3D SIMPLIFICADO  20-Apr-98   11:03:02
*NODE, SYSTEM=R
*ELEMENT,TYPE=C3D4    ,ELSET=GR1
*ELEMENT,TYPE=C3D6    ,ELSET=GR2
*ELEMENT,TYPE=C3D8   ,ELSET=GR3
*ELEMENT,TYPE=C3D8,ELSET=EAPOYO
**
*ELSET,ELSET=MECANOB
GR1,GR2,GR3
**
*ELSET,ELSET=TODOE
GR1,GR2,GR3,EAPOYO
**
**
**
*NSET,NSET=APOYOS
*NSET,NSET=CARABDUC
*NSET,NSET=vastusla
*NSET,NSET=vastusme
*NSET,NSET=contacto
*NSET,NSET=NBOUNDARY
APOYOS,CARABDUC,vastusla,vastusme,contacto
*ELSET,ELSET=FRON4
*NSET,NSET=TODON
**
*ELSET,ELSET=MITAD2
*ELSET,ELSET=MITAD2MECAN
**
**
**	MATERIALES
**
*SOLID SECTION,ELSET=TODOE,MATERIAL=MAT1
*MATERIAL, NAME=MAT1
*USER DEFINED FIELD
*USER MATERIAL, CONSTANTS=16
*DEPVAR
**
*INITIAL CONDITIONS,TYPE=FIELD
**
*BOUNDARY
APOYOS,1,3
**
**
*AMPLITUDE,DEFINITION=TABULAR,INPUT=37,NAME=LC1
*AMPLITUDE,DEFINITION=TABULAR,INPUT=38,NAME=LC2
*AMPLITUDE,DEFINITION=TABULAR,INPUT=36,NAME=LC3
**
**
**
*STEP,AMPLITUDE=STEP,INC=50
*STATIC,DIRECT
1,50
**andar
CARABDUC,1,35.93
CARABDUC,3,72.67
CARABDUC,2,53.54
vastusla,1,-19.37
vastusla,2,11.32
vastusla,3,-85.1
contacto,1,-35.39
contacto,2,-51.89
contacto,3,-165.42
**estar de pie
CARABDUC,1,42.14
CARABDUC,3,113.55
CARABDUC,2,83.58
vastusla,1,-12.93
vastusla,2,9.83
vastusla,3,-81.11
contacto,1,-7.68
contacto,2,-50.12
contacto,3,-184
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contacto,1,-35.3866666667
contacto,2,-51.895
contacto,3,-166
**subir escaleras
*CLOAD,AMPLITUDE=LC2
CARABDUC,1,30.8277777778
CARABDUC,3,78
CARABDUC,2,66.8166666667
CARABDUC,1,8.45777777778
CARABDUC,3,14
CARABDUC,2,10.5977777778
CARABDUC,1,-1.24111111111
CARABDUC,3,-22
CARABDUC,2,-1.13333333333
vastusla,1,-26.16
vastusla,2,13.2477777778
vastusla,3,-127
contacto,1,-32.505
contacto,2,-80.0891666667
contacto,3,-176
vastusme,1,-51.2888888889
vastusme,2,20.1188888889
vastusme,3,-250
**estar de pie
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contacto,1,-7.68166666667
contacto,2,-50.1216666667
contacto,3,-184
*RESTART,WRITE,FREQUENCY=50
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=5
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
**
**
*STEP,AMPLITUDE=STEP,INC=50
*STATIC,DIRECT
1,50
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contacto,1,-35.3866666667
contacto,2,-51.895
contacto,3,-166
*CLOAD,AMPLITUDE=LC2
CARABDUC,1,30.8277777778
CARABDUC,3,78
CARABDUC,2,66.8166666667
CARABDUC,1,8.45777777778
CARABDUC,3,14
CARABDUC,2,10.5977777778
CARABDUC,1,-1.24111111111
CARABDUC,3,-22
CARABDUC,2,-1.13333333333
vastusla,1,-26.16
vastusla,2,13.2477777778
vastusla,3,-127
contacto,1,-32.505
contacto,2,-80.0891666667
contacto,3,-176
vastusme,1,-51.2888888889
vastusme,2,20.1188888889
vastusme,3,-250
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contacto,1,-7.68166666667
contacto,2,-50.1216666667
contacto,3,-184
*RESTART,WRITE,FREQUENCY=50
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=5
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
**
**
*STEP,AMPLITUDE=STEP,INC=50
*STATIC,DIRECT
1,50
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contacto,1,-35.3866666667
contacto,2,-51.895
contacto,3,-166
*CLOAD,AMPLITUDE=LC2
CARABDUC,1,30.8277777778
CARABDUC,3,78
CARABDUC,2,66.8166666667
CARABDUC,1,8.45777777778
CARABDUC,3,14
CARABDUC,2,10.5977777778
CARABDUC,1,-1.24111111111
CARABDUC,3,-22
CARABDUC,2,-1.13333333333
vastusla,1,-26.16
vastusla,2,13.2477777778
vastusla,3,-127
contacto,1,-32.505
contacto,2,-80.0891666667
contacto,3,-176
vastusme,1,-51.2888888889
vastusme,2,20.1188888889
vastusme,3,-250
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contacto,1,-7.68166666667
contacto,2,-50.1216666667
contacto,3,-184
*RESTART,WRITE,FREQUENCY=50
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=5
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
**
**
*STEP,AMPLITUDE=STEP,INC=50
*STATIC,DIRECT
1,50
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contacto,1,-35.3866666667
contacto,2,-51.895
contacto,3,-166
*CLOAD,AMPLITUDE=LC2
CARABDUC,1,30.8277777778
CARABDUC,3,78
CARABDUC,2,66.8166666667
CARABDUC,1,8.45777777778
CARABDUC,3,14
CARABDUC,2,10.5977777778
CARABDUC,1,-1.24111111111
CARABDUC,3,-22
CARABDUC,2,-1.13333333333
vastusla,1,-26.16
vastusla,2,13.2477777778
vastusla,3,-127
contacto,1,-32.505
contacto,2,-80.0891666667
contacto,3,-176
vastusme,1,-51.2888888889
vastusme,2,20.1188888889
vastusme,3,-250
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contacto,1,-7.68166666667
contacto,2,-50.1216666667
contacto,3,-184
*RESTART,WRITE,FREQUENCY=50
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=5
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
**
**
*STEP,AMPLITUDE=STEP,INC=50
*STATIC,DIRECT
1,50
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contacto,1,-35.3866666667
contacto,2,-51.895
contacto,3,-166
*CLOAD,AMPLITUDE=LC2
CARABDUC,1,30.8277777778
CARABDUC,3,78
CARABDUC,2,66.8166666667
CARABDUC,1,8.45777777778
CARABDUC,3,14
CARABDUC,2,10.5977777778
CARABDUC,1,-1.24111111111
CARABDUC,3,-22
CARABDUC,2,-1.13333333333
vastusla,1,-26.16
vastusla,2,13.2477777778
vastusla,3,-127
contacto,1,-32.505
contacto,2,-80.0891666667
contacto,3,-176
vastusme,1,-51.2888888889
vastusme,2,20.1188888889
vastusme,3,-250
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contacto,1,-7.68166666667
contacto,2,-50.1216666667
contacto,3,-184
*RESTART,WRITE,FREQUENCY=50
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=5
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**
**
**
*STEP,AMPLITUDE=STEP,INC=50
*STATIC,DIRECT
1,50
**andar
*CLOAD,AMPLITUDE=LC1
CARABDUC,1,39.4644444444
CARABDUC,3,77
CARABDUC,2,42.0188888889
CARABDUC,1,-2.40555555556
CARABDUC,3,12
CARABDUC,2,12.1711111111
CARABDUC,1,-1.12555555556
CARABDUC,3,-18
CARABDUC,2,-0.65
vastusla,1,-19.3666666667
vastusla,2,11.3188888889
vastusla,3,-86
contacto,1,-35.3866666667
contacto,2,-51.895
contacto,3,-166
*CLOAD,AMPLITUDE=LC2
CARABDUC,1,30.8277777778
CARABDUC,3,78
CARABDUC,2,66.8166666667
CARABDUC,1,8.45777777778
CARABDUC,3,14
CARABDUC,2,10.5977777778
CARABDUC,1,-1.24111111111
CARABDUC,3,-22
CARABDUC,2,-1.13333333333
vastusla,1,-26.16
vastusla,2,13.2477777778
vastusla,3,-127
contacto,1,-32.505
contacto,2,-80.0891666667
contacto,3,-176
vastusme,1,-51.2888888889
vastusme,2,20.1188888889
vastusme,3,-250
*CLOAD,AMPLITUDE=LC3
CARABDUC,1,41.2488888889
CARABDUC,3,113
CARABDUC,2,83.5788888889
vastusla,1,-12.9266666667
vastusla,2,9.83111111111
vastusla,3,-82
contacto,1,-7.68166666667
contacto,2,-50.1216666667
contacto,3,-184
*RESTART,WRITE,FREQUENCY=50
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=5
*NODE OUTPUT,NSET=NBOUNDARY
RF,CF,TF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*EL FILE, ELSET=TODOE,FREQUENCY=1
IVOL,SDV
*END STEP
**