*RESTART,READ
**
*NSET,NSET=CAR2
*NSET,NSET=CAR3
*NSET,NSET=BASE,GENERATE
*NSET,NSET=REACCIONES
**
*INITIAL CONDITIONS,TYPE=FIELD
*BOUNDARY
APOYOS,1,3
**
*STEP,AMPLITUDE=STEP,INC=1
*STATIC,DIRECT
1,1
**adduccion
CAR3,3,-54.22
CAR3,2,-41.62
CAR3,1,-77.30
CARABDUC,1,28.98
CARABDUC,3,41.0
CARABDUC,2,13.78
*RESTART,WRITE,FREQUENCY=1
*NODE PRINT,FREQUENCY=0
*EL PRINT,FREQUENCY=0
*OUTPUT,FIELD,FREQ=1
*NODE OUTPUT,NSET=TODON
RF,CF
*ELEMENT OUTPUT, ELSET=TODOE
S,E,SDV
*END STEP
**
**